**CUSTOM EQUALIZER**

* write equalizer function, which will take db1, …, dbN as argument and will return |X| (amplitude response of obtained filter)
* Apply above defined funciton to the signal with overlap add technique