1. Record your voice or take a recording which has no reverberation.
2. Convert to .wav 16khz.
3. Write a script which will take a recording, apply all filters of reverberation\_impulse\_responses directory to that recording and saves output signals in another folder.

Note that each time you have to convolve your input signal with impulse response, adjust the scale of output audio to fall in int16 range then save new file.